For 1990-2009 cars

## Low and High Beams Inoperative Hatchback

#### Diagnostic Aids

If there are several other symptoms, including an inoperative radiator fan, the windshield washer pump, or the turn signal lamps, inspect ground G102 and G104.

Step | Action | Yes | No
--- | --- | --- | ---
1 | Test fuses EF18, EF23, EF24, EF25, EF26, and EF19. Are any fuses open? | Go to Step 2 | Go to Step 4
2 |

1. Test for a short circuit and repair, if necessary.
2. Replace the fuse.

Is the repair complete?

Go to Step 3

--

3 | Turn ON the low beam headlamps. Do the low beam headlamps work? | Go to Step 6 | Go to Step 4
4 | Inspect the low beam headlamps system. Refer to Low Beams Inoperative . Is any problem found? | Go to Step 5 | --
5 | Repair the problem. Is the repair complete? | Go to Step 6 | --
6 | Turn ON the high beam headlamps. Do the high beam headlamps work? | System OK | Go to Step 7
7 | Inspect the high beam headlamps system. Is any problem found? | Go to Step 8 | --
8 | Repair the problem. Is the repair complete? | System OK | --