For 1990-2009 cars

## Inner Belt Sealing Strip Replacement Notchback

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Straighten the retaining tabs in order to release the channel molding to the door trim panel.
3. Remove the channel molding.

### Installation Procedure

1. Install the channel molding onto the door trim panel.
2. Bend the retaining tabs to secure the channel molding to the door trim panel.
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .