For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Door Trim Panel Replacement .
2. Remove the outside channel molding. Refer to Rear Side Door Window Channel Replacement .
3. Remove the interior rear door garnish molding.
4. Remove the screws and the exterior rear door garnish molding.
5. Remove the door seal trim. Refer to Door Water Deflector Replacement .
6. Remove the screws that secure the glass to the window regulator.
7. Remove the bolts and the guide rail.
8. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the guide rail and the bolts.

Tighten
Tighten the guide rail bolts to 7 N·m (62 lb in).

3. Position the glass within the window regulator.
4. Install the glass screws.

Tighten
Tighten the door glass screws to 7 N·m (62 lb in).

5. Install the door seal trim. Refer to Door Water Deflector Replacement .
6. Install the exterior rear door garnish molding with the screws.

Tighten
Tighten the exterior rear door garnish molding screws to 1.5 N·m (13 lb in).

7. Install the interior rear door garnish molding.
8. Install the outside channel molding. Refer to Rear Side Door Window Channel Replacement .
9. Install the rear door trim panel. Refer to Rear Door Trim Panel Replacement .