For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front left wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the bolts and the front wheel well splash shield.
4. Disconnect the washer hoses from the reservoir.
5. Disconnect the reservoir pump electrical connectors.
6. Remove the bolts, the nuts and the reservoir.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the reservoir with the nuts and the bolts.

Tighten
Tighten the washer fluid reservoir nuts and bolts to 9 N·m (80 lb in).

2. Connect the reservoir pump electrical connectors.
3. Connect the washer hoses to the reservoir.
4. Install the front wheel well splash shield with the bolts.

Tighten
Tighten the front wheel well splash shield bolts to 1.5 N·m (13 lb in).

5. Install the front left wheel. Refer to Tire and Wheel Removal and Installation.
6. Connect the negative battery cable.