For 1990-2009 cars

### Removal Procedure

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

1. Raise and support the vehicle.
2. Disconnect the brake lines from the brake hoses at the body and the rear axle brackets.
3. Remove both brake hose E-ring retainers.
4. Remove the brake hoses from the brackets.

### Installation Procedure

1. Install the brake hoses to the body and the rear axle brackets.

Notice: Refer to Fastener Notice in the Preface section.

2. Connect the brake lines to the brake hose.

Tighten
Tighten the brake lines to 16 N·m (12 lb ft).

3. Install the brake hose retainers.
4. Lower the vehicle.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .
6. Check the brake system for leaks.