For 1990-2009 cars

## Rear Door Trim Panel Replacement Hatchback

#### Tools Required

J 21104-B (KM 475-B) Weatherstrip Remover Universal

### Removal Procedure

1. Lower the rear window.
2. Remove the rear window regulator handle. Refer to Door Window Regulator Handle Replacement .
3. Remove the door pull screw.
4. Remove the inside door handle.
5. Remove the rear door interior garnish molding.
6. Remove the screws at the base of the trim panel.
7. Pry off the trim panel using the trim remover J 21104-B (1).

### Installation Procedure

1. Install the trim panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws at the base of the trim panel.

Tighten
Tighten the trim panel screws to 3.5 N·m (31 lb in).

3. Install the rear door interior garnish molding.
4. Install the inside door handle.
5. Install the door pull screw.

Tighten
Tighten the door pull screw to 3.5 N·m (31 lb in).

6. Install the rear window regulator handle. Refer to Door Window Regulator Handle Replacement .
7. Raise the window.

## Rear Door Trim Panel Replacement Notchback

### Removal Procedure

1. Lower the rear window.
2. Remove the rear window regulator handle. Refer to Door Window Regulator Handle Replacement .
3. Remove the door pull screw.
4. Remove the inside door handle.
5. Remove the rear door interior garnish molding.
6. Remove the screws at the base of the trim panel.
7. Pry off the trim panel.

### Installation Procedure

1. Install the trim panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screws at the base of the trim panel.

Tighten
Tighten the trim panel screws to 3.5 N·m (31 lb in).

3. Install the rear door interior garnish molding.
4. Install the inside door handle.
5. Install the door pull screw.

Tighten
Tighten the door pull screw to 3.5 N·m (31 lb in).

6. Install the rear window regulator handle. Refer to Door Window Regulator Handle Replacement .
7. Raise the window.