For 1990-2009 cars

### Removal Procedure

1. Pull the rear seat knob and fold the rear seat cushion.
2. Remove the bolts and the seat belt anchors.
3. Remove the left rear cargo area trim panel and remove the bolt from the rear center seat belt retractor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt anchors with the bolts.

Tighten
Tighten the seat belt anchor bolts to 38 N·m (28 lb ft).

2. Install the rear center seat belt retractor with the bolt.

Tighten
Tighten the rear center seat belt retractor bolt to 38 N·m (28 lb ft).

3. Install the rear cargo area trim panel and unfold the rear seat.