For 1990-2009 cars

## Parking Lamps and Taillamps Inoperative Hatchback

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Test the headlamps. Do the headlamps work? | -- | Go to Step 3 | Go to Step 2
2 | Repair the headlamps before continuing with this chart. After the headlamps have been repaired, are the parking lamps and tail lamps still inoperative? | -- | Go to Step 3 | System OK
3 |

1. Turn ON the parking lamps.
2. Use a voltmeter to measure the voltage at the bulb socket positive terminal.

Does the voltage at the bulb socket equal the specified value?

11-14 V

Go to Step 4

Go to Step 7

4 | Connect an ohmmeter between ground and the lamp socket negative terminal. Does the ohmmeter indicate continuity? | -- | Go to Step 6 | Go to Step 5
5 | Repair the ground circuit for the lamps. Is the repair complete? | -- | System OK | --
6 | Replace the faulty bulbs. Is the repair complete? | -- | System OK | --
7 | Test fuses EF15 and EF14. Are any of the fuses open? | -- | Go to Step 8 | Go to Step 9
8 |

1. Test for a short circuit and repair, if necessary.
2. Replace the fuse.

Is the repair complete?

--

System OK

--

9 |

1. Turn ON the headlamps.
2. Measure the voltage at fuses EF14, left-side illumination lamp, and EF15, right-side illumination lamp.

Does the voltage at the fuses equal the specified value?

11-14 V

Go to Step 10

--

10 | Repair the open circuit between the fuses EF14 and EF15 and the illumination lamps. Is the repair complete? | -- | System OK | --