For 1990-2009 cars

## Maintenance Schedule Except Europe,North America

### Normal Vehicle Use

These schedules apply to vehicles that are used in the following manner:

• | Carry passengers and cargo within recommended limits

• | Are driven on reasonable road surfaces within legal driving limits

The services shown in this schedule should continue to be performed at the same intervals after 120 000 km (72,000 mi).

### Footnotes

(1) Change the engine oil and the oil filter every 5 000 km (3,000 mi) or every 3 months, whichever comes first, if the vehicle is operated under any of the following conditions:

• | Short distance driving

• | Extensive idling

• | Driving on dusty roads

(2) Inspect the air cleaner element every 7 500 km (4,500 mi) or 3 months if driving under dusty conditions. If necessary, correct, clean, or replace.

(3) Refer to Fluid and Lubricant Recommendations .

(4) Change the brake/clutch fluid every 15 000 km (9,000 mi) if the vehicle is mainly driven in hilly or mountainous terrain, or towing a trailer/caravan frequently.

(5) More frequent maintenance is required if the vehicle is mainly used in short distance driving, extended idling, frequent low speed operation in stop-start traffic, or driving in dusty conditions.

(6) Rotate and balance wheels, if necessary.

(7) Change the automatic transaxle fluid every 60 000 km (36,000 mi) if the vehicle is mainly driven under any of the following severe conditions:

• | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher

• | In hilly or mountainous terrain

• | Doing frequent trailer towing

• | Used for taxi, police or delivery service

### 1 000 km (600 mi)

• | Inspect the engine oil and oil filter. Refer to footnotes (1), (3).

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the parking brake.

• | Inspect the automatic transaxle fluid, Refer to footnote (3).

• | Inspect the tire condition and inflation pressure.

• | Inspect wheel alignment. Refer to footnote (6).

• | Inspect the power steering fluid and lines. Refer to footnote (1).

### 15 000 km (9,000 mi) or Every 12 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs for the 1.6 DOHC engine.

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake pads and disc or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Inspect the manual transaxle. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3), (5), (7).

• | Inspect the chassis and underbody bolts and nuts tight/secure.

• | Inspect the tire condition and inflation pressure.

• | Inspect wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 30 000 km (18,000 mi) or Every 24 Months, Whichever Comes First

• | Inspect the drive belts - alternator, power steering and A/C belt.

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs for the 1.6 DOHC engine.

• | Inspect spark plugs for the 1.8 DOHC engine.

• | Inspect the PCV system.

• | Inspect the timing belt.

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and disc or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and the connections, including the booster.

• | Inspect manual transaxle oil. Refer to footnote (3).

• | Inspect automatic transaxle fluid. Refer to footnotes (3), (5), (7).

• | Inspect the chassis and underbody bolts and nuts tight/secure.

• | Inspect tire condition and inflation pressure.

• | Inspect wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect power steering fluid and lines. Refer to footnote (3).

• | Inspect drive shaft boots.

• | Inspect seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 45 000 km (24,000 mi) or Every 24 Months, Whichever Comes First

• | Change engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Change the engine coolant. Refer to footnote (3).

• | Change fuel filter.

• | Inspect the fuel lines and connections.

• | Change the air cleaner element. Refer to footnote (2).

• | Change the spark plug for the 1.6 DOHC engine.

• | Inspect the EVAP canister, vapor lines and solenoid valve filter.

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake drum and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and the connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3), (5), (7).

• | Inspect that the chassis and the underbody bolts and nuts tight/secure.

• | Inspect the tire condition and the inflation pressure.

• | Inspect the wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (1).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 60 000 km (36,000 mi) or Every 48 Months, Whichever Comes First

• | Inspect the drive belts - alternator, power steering, and A/C belt.

• | Change engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect air cleaner element. Refer to footnote (2).

• | Change the spark plugs for the 1.6 DOHC engine.

• | Change the spark plugs for the 1.8 DOHC engine.

• | Inspect the PCV system.

• | Change the timing belt.

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake pads and disc or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and the connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3), (5), (7).

• | Inspect that the chassis and the underbody bolts and nuts tight/secure.

• | Inspect the tire condition and the inflation pressure.

• | Inspect the wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 75 000 km (45,000 mi) or Every 60 Months, Whichever Comes First

• | Change engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs for the 1.6 DOHC engine.

• | Change the interior air filter A/C system.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake pads and disc or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and connections, including booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnote (3).

• | Inspect the chassis and underbody and nuts tight/secure.

• | Inspect tire condition and inflation pressure.

• | Inspect wheel alignment. Refer to footnote (6).

• | Inspect steering wheel and linkage.

• | Inspect power steering fluid and lines. Refer to footnote (3).

• | Inspect drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate locks, hinges and hood latch.

### 90 000 km (54,000 mi) or Every 72 Months, Whichever Comes First

• | Inspect the drive belts - alternator, power steering and A/C belt.

• | Change engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Change the engine coolant. Refer to footnote (3).

• | Change the fuel filter.

• | Inspect the fuel line and connections.

• | Change air cleaner element. Refer to footnote (2).

• | Change the spark plugs for the 1.6 DOHC engine.

• | Change the spark plugs for the 1.8 DOHC engine.

• | Inspect the EVAP canister, vapor line and solenoid valve filter.

• | Inspect the PCV system.

• | Inspect the timing belt.

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake pads and discs or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnotes (3), (5), (7).

• | Inspect that the chassis and underbody bolts and nuts are tight/secure.

• | Inspect the tire condition and inflation pressure.

• | Inspect the wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 105 000 km (63,000 mi) or Every 84 Months, Whichever Comes First

• | Change engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel line and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs for the 1.6 DOHC engine.

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake pads and disc or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnotes (3), (5), (7).

• | Inspect that the chassis and underbody bolts and nuts are tight/secure.

• | Inspect the tire condition and inflation pressure.

• | Inspect the wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 120 000 km (72,000 mi) or Every 96 Months, Whichever Comes First

• | Inspect the drive belts - alternator, power steering and A/C belt.

• | Change engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel line and connections.

• | Inspect air cleaner element. Refer to footnote (2).

• | Change the spark plugs for the 1.6 DOHC engine.

• | Change the spark plugs for the 1.8 DOHC engine.

• | Inspect the PCV system.

• | Change the timing belt.

• | Change the interior air filter A/C system.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and disc. Refer to footnote (5).

• | Inspect the rear brake pads and discs or drums and linings. Refer to footnote (5).

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnotes (3), (5), (7).

• | Inspect that the chassis and underbody bolts and nuts are tight/secure.

• | Inspect the tire condition and inflation pressure.

• | Inspect the wheel alignment. Refer to footnote (6).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

## Maintenance Schedule Europe

### Normal Vehicle Use

These schedules are for vehicles that:

• | Carry passengers and cargo within recommended limits.

• | Are driven on reasonable road surfaces within legal driving limits.

• | Use the recommended fuel.

The services shown in this schedule up to 120 000 km (72,000 mi) should be performed after 120 000 km (72,000 mi) at the same intervals.

### Footnotes

The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance will not nullify the emission warranty or limit recall liability prior to the completion of the vehicles useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

(1) Inspect every 3 000 km (1,900 mi) and replenish engine oil. If the vehicle is operated under severe conditions: short distance driving, extensive idling or driving in dusty conditions, change engine oil every 5 000 km (3,100 mi) or 3 months, whichever comes first.

(2) More frequent maintenance is required if driving in dusty conditions.

(3) Refer to Fluid and Lubricant Recommendations .

(4) Change the brake fluid every 15 000 km (9,000 mi) if the vehicle is mainly driven under severe conditions: driving in hilly or mountainous terrain.

(5) More frequent maintenance is required if used under severe conditions: short distance driving, extended idling, frequent low speed operation in stop-start traffic or driving in dusty conditions.

(6) Rotate and balance wheels, if necessary.

(7) Check the brakes during tire rotation

(8) Inspect every 5 000 km (3,000 mi)

(9) Rotate every 5 000 km (3,000 mi)

(10) Inspect when abnormal condition is noted.

### 1 000 km (600 mi)

• | Inspect the power steering and A/C compressor belt.

• | Inspect the engine oil and oil filter. Refer to footnote (1), (3).

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the brake fluid. Refer to footnote (3), (4).

• | Inspect the parking brake. Refer to footnote (4).

• | Inspect the power steering fluid and lines.

• | Inspect wheel alignment.

### 15 000 km (9,000 mi) or Every 12 Months, Whichever Comes First

• | Inspect the alternator-belt (1.2L SOHC).

• | Inspect the power steering and A/C compressor belt (1.2L SOHC).

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Change the interior air filter A/C.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drums and linings.

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Change the manual transaxle fluid (1.2L SOHC). Refer to footnote (3).

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnote (3).

• | Inspect the chassis and underbody bolts and nuts tight/secure.

• | Inspect the tire condition and inflation pressure. Refer to footnote (6), (8).

• | Inspect wheel alignment. Refer to footnote (10).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines.

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 30 000 km (18,000 mi) or Every 24 Months, Whichever Comes First

• | Inspect the alternator-belt (1.2L SOHC).

• | Inspect the alternator, power steering, and A/C compressor belt.

• | Inspect the power steering, A/C compressor drive belt (1.2L SOHC).

• | Change the engine oil and filter, or every 3 months, whichever occurs first.

• | Inspect the cooling system hoses and connections

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Inspect the PCV system.

• | Inspect the timing belt.

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drums and linings.

• | Inspect the parking brake.

• | Inspect the brake line and the connections, including the booster.

• | Inspect manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnote (3).

• | Inspect the chassis and underbody bolts and nuts tight/secure.

• | Inspect tire condition and inflation pressure. Refer to footnote (6), (8).

• | Rotate tires. Refer to footnote (7), (9).

• | Inspect wheel alignment. Refer to footnote (10).

• | Inspect the steering wheel and linkage.

• | Inspect power steering fluid and lines.

• | Inspect drive shaft boots.

• | Inspect seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 45 000 km (27,000 mi) or Every 36 Months, Whichever Comes First

• | Change the alternator-belt (1.2L SOHC).

• | Inspect the power steering, and A/C compressor belt (1.2L SOHC).

• | Change engine oil and filter, or every 3 months, whichever occurs first.

• | Inspect the cooling system hoses and connections.

• | Change the engine coolant. Refer to footnote (3).

• | Change the fuel filter.

• | Inspect the fuel lines and connections.

• | Change air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Inspect the charcoal canister and vapor lines.

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings. Refer to footnote.

• | Inspect the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drum and linings.

• | Inspect the parking brake.

• | Inspect the brake line and connections, including booster.

• | Change the manual transaxle oil (1.2L SOHC). Refer to footnote (1).

• | Inspect the manual transaxle oil. Refer to footnote (1).

• | Inspect the automatic transaxle oil. Refer to footnote (1).

• | Inspect the chassis and underbody and nuts tight/secure.

• | Inspect tire condition and inflation pressure. Refer to footnote (6), (8).

• | Rotate tires. Refer to footnote (7), (9).

• | Inspect wheel alignment. Refer to footnote (10).

• | Inspect steering wheel and linkage.

• | Inspect power steering fluid and lines.

• | Inspect drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate locks, hinges and hood latch.

### 60 000 km (36,000 mi) or Every 48 Months, Whichever Comes First

• | Inspect the alternator-belt (1.2L SOHC).

• | Inspect the alternator, power steering, and A/C compressor belt.

• | Inspect the power steering, A/C compressor drive belt (1.2L SOHC).

• | Change engine oil and filter, or every 3 months, whichever occurs first. Refer to footnote (1).

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Inspect the PCV system.

• | Change the timing belt.

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drum and linings.

• | Inspect the parking brake.

• | Inspect the brake line and the connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnote (3).

• | Inspect that the chassis and the underbody bolts and nuts tight/secure.

• | Inspect the tire condition and the inflation pressure. Refer to footnote (6), (8).

• | Rotate the tires. Refer to footnote (7), (9).

• | Inspect the wheel alignment. Refer to footnote (10).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines.

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 75 000 km (45,000 mi) or Every 60 Months, Whichever Comes First

• | Inspect the alternator-belt (1.2L SOHC).

• | Change the power steering, and A/C compressor belt (1.2L SOHC).

• | Change the engine oil and filter, or every 3 months, whichever occurs first. Refer to footnote (1).

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drum and linings.

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Change the manual transaxle oil (1.2L SOHC). Refer to footnote (1).

• | Inspect the manual transaxle oil.

• | Inspect the automatic transaxle oil. Refer to footnote (1).

• | Inspect that the chassis and the underbody bolts and nuts are tight/secure.

• | Inspect the tire condition and inflation pressure. Refer to footnote (6), (8).

• | Rotate the tires. Refer to footnote (7), (9).

• | Inspect the wheel alignment. Refer to footnote (10).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines.

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 90 000 km (54,000 mi) or Every 72 Months, Whichever Comes First

• | Change the alternator-belt (1.2L SOHC).

• | Inspect the alternator, power steering, and A/C compressor belt.

• | Inspect the power steering, A/C compressor belt (1.2L SOHC).

• | Change engine oil and filter, or every 3 months, whichever occurs first. Refer to footnote (1).

• | Inspect the cooling system hoses and connections.

• | Change the engine coolant. Refer to footnote (3).

• | Change the fuel filter.

• | Inspect the fuel lines and connections.

• | Change air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Inspect the charcoal canister and vapor lines.

• | Inspect the PCV system.

• | Inspect the timing belt.

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drum and linings.

• | Inspect the parking brake.

• | Inspect the brake line and the connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnote (3).

• | Inspect that the chassis and the underbody bolts and nuts tight/secure.

• | Inspect the tire condition and the inflation pressure. Refer to footnote (6), (8).

• | Rotate the tires. Refer to footnote (7), (9).

• | Inspect the wheel alignment. Refer to footnote (10).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines.

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 105 000 km (63,000 mi) or Every 84 Months, Whichever Comes First

• | Inspect the alternator-belt (1.2L SOHC).

• | Inspect the power steering, and A/C compressor belt (1.2L SOHC).

• | Change engine oil and filter, or every 3 months, whichever occurs first. Refer to footnote (3).

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drum and linings.

• | Inspect the parking brake.

• | Inspect the brake line and connections, including booster.

• | Change the manual transaxle oil (1.2L SOHC). Refer to footnote (3).

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnote (3).

• | Inspect the chassis and underbody and nuts tight/secure.

• | Inspect tire condition and inflation pressure. Refer to footnote (6), (8).

• | Rotate tires. Refer to footnote (7), (9).

• | Inspect wheel alignment. Refer to footnote (10).

• | Inspect steering wheel and linkage.

• | Inspect power steering fluid and lines.

• | Inspect drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate locks, hinges and hood latch.

### 120 000 km (72,000 mi) or Every 96 Months, Whichever Comes First

• | Inspect the alternator-belt (1.2L SOHC).

• | Inspect the alternator, power steering, and A/C compressor belt.

• | Inspect the power steering, A/C compressor belt (1.2L SOHC).

• | Change engine oil and filter, or every 3 months, whichever occurs fir Refer to footnote (3).

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the valve clearance (1.2L SOHC).

• | Inspect the PCV system.

• | Change the timing belt.

• | Change the interior air filter.

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnote (3), (4).

• | Inspect the front brake pads and disc.

• | Inspect the brake drum and linings.

• | Inspect the parking brake.

• | Inspect the brake line and connections, including the booster.

• | Inspect the manual transaxle oil. Refer to footnote (3).

• | Inspect the automatic transaxle oil. Refer to footnote (3).

• | Inspect that the chassis and underbody bolts and nuts are tight/secure.

• | Inspect the tire condition and inflation pressure. Refer to footnote (6), (8).

• | Rotate the tires. Refer to footnote (7), (9).

• | Inspect the wheel alignment. Refer to footnote (10).

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines.

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

## Maintenance Schedule North American Emissions

The Maintenance Schedule information will only be found in the Owner's Manual.

Refer to the Maintenance Schedule subsection of the Owner's Manual, or you may be able to use the Search information function using the words Scheduled Maintenance.

## Maintenance Schedule Mexico

### Normal Vehicle Use

These schedules apply to vehicles that are used in the following manner:

• | Carry passengers and cargo within recommended limits.

• | Are driven on reasonable road surfaces within legal driving limits.

The services shown in this schedule should continue to be performed at the same intervals after 100,000 km (60,000 mi).

### Footnotes

(1) Change the engine oil and the oil filter every 5,000 km (3,000 mi) or every 3 months, whichever comes first, if the vehicle is operated under any of the following conditions:

• | Short distance driving.

• | Extensive idling.

• | Driving on dusty roads.

(2) Inspect the air cleaner element every 5,000 km (3,000 miles) or 3 months if driving on dusty roads. If necessary, correct, clean or replace.

(3) Refer to Fluid and Lubricant Recommendations .

(4) Change the brake/clutch fluid every 15,000 km (9,000 mi) if the vehicle is mainly driven under the following severe conditions: driving in hilly or mountainous terrain, or towing a trailer/caravan frequently.

(5) More frequent maintenance is required if under severe conditions: short distance driving, extensive idling, frequent low speed operation in stop-start traffic or driving on dusty roads.

(6) More frequent maintenance is required if under dusty driving conditions.

(7) If engine coolant is DEX-COOL®, change it every 5 years or 240,000 km (150,000 miles).

### 10 000 km (6,000 mi) or Every 6 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the interior air filter if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnotes (5).

• | Inspect the rear brake pads and discs or drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnote (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 20 000 km (12,000 mi) or Every 12 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Change the interior air filter if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and the connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 30 000 km (18,000 mi) or Every 18 Months, Whichever Comes First

• | Inspect the drive belts for the alternator, the power steering pump, and the A/C compressor, if equipped.

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the PCV system.

• | Inspect the timing belt.

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 40 000 km (24,000 mi) or Every 24 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Change the engine coolant. Refer to footnote (3), (7).

• | Change the fuel filter.

• | Inspect the fuel lines and connections.

• | Change the air cleaner element. Refer to footnote (2).

• | Inspect the EVAP canister, the vapor lines, and the solenoid valve filter.

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or the drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and the connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and the underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 50 000 km (30,000 mi) or Every 30 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or the drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and the underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 60 000 km (36,000 mi) or Every 36 Months, Whichever Comes First

• | Inspect the drive belts for the alternator, the power steering pump, and the A/C compressor, if equipped.

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the PCV system.

• | Change the timing belt.

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or the drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and the connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and the underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 70 000 km (42,000 mi) or Every 42 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and disc or drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate locks, hinges and hood latch.

### 80 000 km (48,000 mi) or Every 48 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Change the engine coolant. Refer to footnote (3), (7).

• | Change the fuel filter.

• | Inspect the fuel lines and connections.

• | Change the air cleaner element. Refer to footnote (2).

• | Inspect the spark plugs.

• | Inspect the EVAP canister, the vapor lines, and the solenoid valve filter.

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or the drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 90 000 km (54,000 mi) or Every 54 Months, Whichever Comes First

• | Inspect the drive belts for the alternator, the power steering pump, and the A/C compressor, if equipped.

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the spark plugs.

• | Inspect the PCV system.

• | Inspect the timing belt.

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Change the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or the drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.

### 100 000 km (60,000 mi) or Every 60 Months, Whichever Comes First

• | Change the engine oil and filter. Refer to footnotes (1), (3).

| An Emission Control Service.

• | Inspect the cooling system hoses and connections.

• | Inspect the engine coolant. Refer to footnote (3).

• | Inspect the fuel lines and connections.

• | Inspect the air cleaner element. Refer to footnote (2).

• | Change the interior air filter, if equipped with A/C. Refer to footnote (6).

• | Inspect the exhaust pipes and mountings.

• | Inspect the brake/clutch fluid. Refer to footnotes (3), (4).

• | Inspect the front brake pads and discs. Refer to footnote (5).

• | Inspect the rear brake pads and discs or the drums and linings. Refer to footnote (5).

• | Inspect the park brake.

• | Inspect the brake lines and connections, including the booster.

• | Inspect the manual transaxle fluid. Refer to footnote (3).

• | Inspect the automatic transaxle fluid. Refer to footnotes (3).

• | Inspect the chassis and underbody bolts and nuts.

• | Inspect the steering wheel and linkage.

• | Inspect the power steering fluid and lines. Refer to footnote (3).

• | Inspect the drive shaft boots.

• | Inspect the seat belts, buckles and anchors.

• | Lubricate the locks, hinges and hood latch.