For 1990-2009 cars

## Shoulder Belt Replacement - Rear Notchback

### Removal Procedure

1. Remove the bolt (1) and the seat belt anchor on the wheelhouse trim panel.
2. Remove the upper back panel shelf. Refer to Rear Window Shelf Trim Panel Replacement.
3. Remove the bolt (1) and the seat belt retractor (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt retractor (2) with the bolt (1) and tighten to 38 N·m (28 lb ft).
2. Install the upper back panel shelf. Refer to Rear Window Shelf Trim Panel Replacement.
3. Install the seat belt anchor to the upper wheelhouse trim panel with the bolt (1) and tighten to 38 N·m (28 lb ft).

## Shoulder Belt Replacement - Rear Hatchback

### Removal Procedure

1. Remove the bolt (1) and the seat belt lower anchor.
2. Remove the luggage compartment wheel house trim panel.
3. Remove the bolt and the seat belt retractor.
4. Remove the screws (3) and the load floor rear compartment trim panel.
5. Remove the bolt (1) and the seat belt upper anchor (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt retractor with the bolt and tighten to 38 N·m (28 lb ft).
2. Install the luggage compartment wheel house trim panel.
3. Install the bolt (1) and the seat belt upper anchor (2) and tighten to 38 N·m (28 lb ft).
4. Install the load floor rear compartment trim panel. Secure with the screws (3).
5. Install the seat belt lower anchor with the bolt (1) and tighten to 38 N·m (28 lb ft).