For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the breather hose from the valve cover.
3. Remove the eight bolts from the valve cover.
4. Remove the valve cover.
5. Remove the valve cover gasket.
6. Clean the sealing surfaces.

### Installation Procedure

1. Install the new valve cover gasket and the valve cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the eight bolts to the valve cover.

Tighten
Tighten the valve cover bolts to 9 N·m (80 lb in).

3. Connect the breather tube to the valve cover.
4. Connect the negative battery cable.