For 1990-2009 cars

## Rear Compartment Lid Lock Cylinder Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the clips and the rear compartment lid trim.
3. Disconnect the electrical connector.
4. Disconnect the lock rod.
5. Remove the bolt and the lock cylinder.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the lock cylinder with the bolt and tighten to 4 N·m (35 lb in).
2. Connect the lock rod.
3. Install the rear compartment lid trim with the clips.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Rear Compartment Lid Lock Cylinder Replacement Hatchback

### Removal Procedure

1. Remove the hatchback door lower garnish molding, if equipped.
2. Disconnect the lock rod.
3. Remove the nuts and the lock cylinder.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the lock cylinder with the nuts and tighten to 3 N·m (27 lb in).
2. Connect the lock rod.
3. Install the hatchback door lower garnish molding, if equipped.