For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical exhaust gas recirculation (EGR) valve electrical connector.
3. Remove the EGR valve retaining bolts.
4. Remove the EGR valve.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the EGR valve with the bolts.

Tighten
Tighten the electrical EGR valve retaining bolts to 30 N·m (22 lb ft).

2. Connect the EGR valve electrical connector.
3. Connect the negative battery cable.