For 1990-2009 cars

## High Mount Stop Lamp Replacement Rear Spoiler

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the spoiler. Refer to Rear Spoiler Replacement.
3. Remove the screws and the spoiler CHMSL.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the spoiler CHMSL with the screws and tighten to 3 N·m (27 lb in).
3. Install the spoiler. Refer to Rear Spoiler Replacement.
4. Connect the negative battery cable.

## High Mount Stop Lamp Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Open the rear deck lid.
3. Remove the screws and the center high-mounted stop lamp (CHMSL).
4. Remove the CHMSL bulb.

### Installation Procedure

1. Install the CHMSL bulb.
2. Install the CHMSL with the screws.
3. Connect the negative battery cable.

## High Mount Stop Lamp Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Open the hatchback door.
3. Pry open the center high-mounted stop lamp (CHMSL) access cover with a screwdriver.
4. Disconnect the electrical connector.
5. Remove the screws and the CHMSL.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the CHMSL with the screws and tighten to 3 N·m (27 lb in).
2. Connect the electrical connector.
3. Close the CHMSL access cover.
4. Connect the negative battery cable.