For 1990-2009 cars

Important: The following steps must be completed before using the symptom tables.

Perform the Diagnostic System Check - Vehicle before using the Symptom tables in order to verify that there are no DTCs set.

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the Power Sunroof System.

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

### Intermittent

Faulty electrical connections or wiring may be the cause of intermittent conditions.

### Symptom List

Refer to a symptom diagnostic procedure from the following list in order to diagnose the symptom:

• | Door Open Warning Chime Inoperative

• | Key Reminder Chime Inoperative

• | Clock Malfunction

• | Engine Coolant Temperature Gage Inaccurate or Inoperative

• | Fuel Gage Inaccurate or Inoperative

• | Speedometer and/or Odometer Inaccurate or Inoperative

• | Chime Inoperative