For 1990-2009 cars

#### Special Tools

KM-6009 Remover/Installer

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Detach the ignition coil cover.
3. Disconnect the ignition coil connector.
4. Remove the ignition coil bolts (1).
5. Install the KM-6009 .
6. Remove the ignition coil (2).

### Installation Procedure

1. Install the ignition coil (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the ignition coil bolts (1).

Tighten
Tighten the ignition coil bolts to 8 N·m (70.8 lb in).

3. Connect the ignition coil connector.
4. Install the ignition coil cover.
5. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.