For 1990-2009 cars

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the breather hose.
3. Loosen the clamp and disconnect outlet tube (1).
4. Remove the air cleaner assembly bolts (1).
5. Remove the air cleaner assembly (2).

### Installation Procedure

1. Install the air cleaner assembly (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the air cleaner assembly bolts (1) and tighten to 6 N·m (4.4 lb ft).
3. Connect the air cleaner outlet tube (1) and tighten the clamp.
4. Connect the breather hose.
5. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.