For 1990-2009 cars

### Removal Procedure

1. Remove the crossmember assembly. Refer to Front Suspension Crossmember Replacement.
2. Remove the stabilizer bar from the crossmember assembly by removing the U-clamp bolts.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the U-clamps and the stabilizer bar to the crossmember and tighten to 25 N·m (18 lb ft).
2. Install the crossmember assembly. Refer to Front Suspension Crossmember Replacement.