For 1990-2009 cars

### Removal Procedure

Notice: Refer to Liftgate Assist Rod Notice in the Preface section.

1. Open and suitably support the hatchback door.
2. Unscrew and remove the gas support assembly from the hatchback door and the body.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the gas support assembly onto the hatchback door and the body.

Tighten
Tighten the gas support assembly studs to 8 N·m (71 lb in).

2. Close the hatchback door.