For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Slide the side turn signal lamp rearward.
3. Remove the lamp.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the side turn signal lamp.
3. Connect the negative battery cable.