For 1990-2009 cars

System | DTCs Required to Set System Status to YES
--- | ---
If an I/M System Status indicator did NOT update to YES during the Inspection/Maintenance (I/M) Complete System Set Procedure , review each indicator and reference this table to determine each DTC associated with the I/M System Status Indicator. Each DTC listed below has specific conditions that must be met for the diagnostic to run. Included within the conditions are additional DTCs, which if set, may inhibit the DTCs listed below from running. Reviewing and operating the vehicle within the Conditions for Running for each DTC listed below will allow the I/M System Status Indicators to transition to YES.
Catalyst Monitor | DTC P0420 --Refer to DTC P0420.
Evaporative Emission (EVAP) |

• | DTC P0442--Refer to DTC P0442.

• | DTC P0446--Refer to DTC P0446.

• | DTC P0455--Refer to DTC P0455.

• | DTC P0496--Refer to DTC P0496.

Oxygen Sensor |

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140--Refer to DTC P0131, P0132, P0134, P0137, P0138, or P0140.

• | DTC P0133 or P1133--Refer to DTC P0133 or P1133.

• | DTC P2270--Refer to DTC P2270.

• | DTC P2271--Refer to DTC P2271.

• | DTC P2A00--Refer to DTC P2A00.

Oxygen Sensor Heater | DTC P0030, P0036, P0053, P0054, P0135, or P0141--Refer to DTC P0030, P0036, P0053, P0054, P0135, or P0141.