For 1990-2009 cars

#### Special Tools

• | J 8062 Valve Spring Compressor - Head Off

• | J 36017 Valve Seal Remover

• | J 43963 Valve Spring Compressor (Off Car)

For equivalent regional tools, refer to Special Tools

1. Remove the intake camshaft position sensor and bolt.

Note: Ensure that the valve train components are kept together and identified in order for proper installation in their original position.

2. Using the J 8062 compressor and the J 43963 Valve Spring Compressor (Off Car) , compress the valve spring.
3. Remove the valve keys.
4. Slowly release the J 8062 compressor and the J 43963 Valve Spring Compressor (Off Car) from the valve spring assembly.
5. Remove the retainer.
6. Remove the spring.

Caution: Do not damage the valve guide. Remove any burrs that have formed at the key groove by chamfering the valve stem with an oil stone or a file.

7. Using the J 36017 remover , remove the valve seal. Do not reuse the valve seal.
8. Remove the valve.
9. Remove the remaining valves.
10. Remove the cylinder head plugs.