For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel (I/P) trim plates. Refer to the following procedures:

• | Instrument Panel Center Trim Panel Replacement

• | Instrument Panel Trim Panel Replacement - Left Side

2. Tilt the steering wheel down.

1 | Instrument Panel Cluster Bezel Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.2 N·m (19 lb in)
2 | Panel Cluster Bezel Assembly