For 1990-2009 cars

## Front Wheel Bearing and Hub Replacement L61/LE5

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the brake rotor assembly. Refer to Front Brake Rotor Replacement.
4. Remove the wheel drive shaft assembly from the knuckle. Refer to Wheel Drive Shaft Replacement.

1 | Speed Sensor Electrical Connector
2 | Wheel Bearing/Hub Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 115 N·m (85 lb ft)
3 | Wheel Bearing/Hub Assembly
4 | Wheel Bearing/Hub Spacer

## Front Wheel Bearing and Hub Replacement LSJ

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Remove the brake rotor assembly. Refer to Front Brake Rotor Replacement .
4. Remove the wheel drive shaft assembly from the knuckle. Refer to Wheel Drive Shaft Replacement .

1 | Speed Sensor Electrical Connector
2 | Wheel Bearing/Hub Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 115 N·m (85 lb ft)
3 | Wheel Bearing/Hub Assembly
4 | Wheel Bearing/Hub Spacer