For 1990-2009 cars

The following approximate capacities are given in English and metric conversions. See Fluid and Lubricant Recommendations for more information. All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

Application | Specification
--- | ---
Metric | English
Cooling System

- 2.0L L4 Engine Supercharged - RPO LSJ

5.7 liters

6.0 quarts

- 2.2L L4 Engine - RPO L61

6.5 liters

6.8 quarts

- 2.4L L4 Engine - RPO LE5

7.0 liters

7.4 quarts

Intercooler System 2.0L Engine - RPO LSJ | 1.9 liters | 2.0 quarts
Engine Oil With Filter

- 2.0L L4 Engine Supercharged - RPO LSJ

6.0 liters

6.3 quarts

- 2.2L L4 Engine - RPO L61

4.8 liters

5.0 quarts

- 2.4L L4 Engine - RPO LE5

4.8 liters

5.0 quarts

Fuel Tank | 51.1 liters | 13.5 gallons
Transmission/Transaxle - 4T40-E

- Bottom Pan Removed

6.6 liters

7.0 quarts

- Dry

12.2 liters

12.9 quarts

- Complete Overhaul

9.0 liters

9.5 quarts

- Transaxle, Manual - Getrag 5 Speed

1.7 liters

1.8 quarts

- Transaxle, Manual - MU3

1.9 liters

2.0 quarts