For 1990-2009 cars

### Removal Procedure

1. Remove the right front tire and wheel. Refer to Tire and Wheel Removal and Installation .
2. Remove the right front fender liner. Refer to Front Fender Liner Replacement .
3. Remove the air cleaner intake duct assembly push-in fasteners.
4. Remove the air cleaner intake duct assembly bolt.
5. Remove the intake duct assembly from the vehicle.

### Installation Procedure

1. Position the intake duct assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the intake duct assembly bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb ft).

3. Install the intake duct assembly push in fasteners.
4. Install the right front fender liner. Refer to Front Fender Liner Replacement .
5. Install the right front tire and wheel. Refer to Tire and Wheel Removal and Installation .