For 1990-2009 cars

### Removal Procedure

1. Remove the clutch pedal assembly. Refer to Clutch Pedal Replacement .
2. Disconnect the electrical connector (2) from the clutch pedal position (CPP) switch (1).
3. Rotate the CPP switch (1) counterclockwise to release, and remove the switch from the clutch pedal assembly.

### Installation Procedure

1. A 3/32 inch or 2 mm drill bit can be used as a gage tool for the proper adjustment of the CPP switch. Insert and seat the 3/32 inch or 2 mm drill bit through the slot in the top of the clutch pedal assembly.
2. Install the CPP switch (1) to the clutch pedal assembly.
3. While holding the pedal in the fully released position, press the switch (1) toward the pedal until the barrel of the switch touches the drill bit on the pedal assembly.
4. Rotate the switch (1) clockwise to secure.
5. Remove the drill bit.
6. Connect the electrical connector (2) to the CPP switch (1).
7. Install the clutch pedal assembly. Refer to Clutch Pedal Replacement .