For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Do not strike or jolt the inflatable restraint front end sensor. Before applying power to the front end sensor make sure that it is securely fastened. Failure to observe the correct installation procedure could cause SIR deployment, personal injury, or unnecessary SIR system repairs.

#### Preliminary Procedure

Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.

1 | Forward Discriminating Sensor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Loosen the bolts in order to remove the sensor. Tighten
8 N·m (71 lb in)

2 | Forward Discriminating Sensor

#### Procedure

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connector.