For 1990-2009 cars

### Removal Procedure

1. Remove the left front wheel. Refer to Tire and Wheel Removal and Installation .
2. Disconnect the vehicle speed sensor (VSS) electrical connector (2).
3. Remove the retainer bolt.
4. Remove the retainer.
5. Remove the VSS.
6. Remove and discard the O-ring.

### Installation Procedure

1. Lubricate a new O-ring with transmission fluid. Refer to Lubrication Specifications .
2. Install the new O-ring.
3. Install the VSS retainer.

Install the VSS assembly.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the VSS retainer bolt.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

5. Connect the VSS connector to the VSS (2).
6. Install the left front wheel. Refer to Tire and Wheel Removal and Installation .