For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the condenser bolts.

Important: You are not required to discharge the A/C system.

3. Slide the condenser down to disengage the upper mounting tabs from the radiator. Position the condenser away from the radiator and support the condenser.
4. Remove the right and left radiator side baffles.

### Installation Procedure

1. Install the right and left radiator side baffles.
2. Slide the condenser up to engage the upper mounting tabs into the radiator.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the condenser bolts.

Tighten
Tighten the bolts to 10 N·m (88 lb in).

4. Lower the vehicle.