For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the cushion frame. Refer to Front Seat Cushion Frame Replacement .
3. Remove the seat back cover and pad assembly. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .

1 | Recliner Handle Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 20 N·m (14 lb ft)
2 | Seat Back Recliner Handle Assembly Tip Remove the recliner handle return spring.