For 1990-2009 cars

### Removal Procedure

1. Disconnect the ignition coil connectors from the ignition coils.
2. Remove the retaining bolts from the ignition coils.
3. Remove the ignition coils from the engine.

### Installation Procedure

Important: Make sure that the ignition coil seals are properly seated to the valve cover.

1. Install the ignition coil.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the ignition coil retaining bolts.

Tighten
Tighten the ignition coil retaining bolts to 10 N·m (89 lb in).

3. Replace the ignition coil connectors.