For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Camshaft Position Sensor Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Camshaft Position Sensor O-ring

#### Procedure

Lubricate the camshaft position sensor O-ring seal with clean engine oil.

3 | Camshaft Position Sensor (Intake CMP shown, exhaust CMP similar)

#### Procedure

1. Disconnect the sensor harness connector.
2. Inspect the camshaft position sensor for damage, replace as necessary.