For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear spring. Refer to Coil Spring Replacement .
3. Remove the coil spring insulator from the rear axle assembly.

### Installation Procedure

1. Install the coil spring insulator to the rear axle assembly.
2. Install the rear spring, taking care to properly seat the spring to the insulator. Refer to Coil Spring Replacement .
3. Lower the vehicle.