For 1990-2009 cars

## Front Side Door Window Regulator Replacement Manual Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Side Door Window Regulator Bolt (Qty: 5) Tighten 10 N·m (89 lb in)
3 | Front Side Door Window Regulator Assembly

## Front Side Door Window Regulator Replacement Manual Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Bolts (Qty: 5) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Window Regulator Assembly

## Front Side Door Window Regulator Replacement Power Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Side Door Window Regulator Bolt (Qty: 5) Tighten 10 N·m (89 lb in)
3 | Front Side Door Window Regulator Assembly Tip Disconnect the electrical connector.

## Front Side Door Window Regulator Replacement Power Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Bolts (Qty: 5) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Window Regulator Assembly Tip Disconnect the electrical connector.