For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Fold the rear seat down.
2. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement.
3. Remove the upper quarter trim panel assembly. Refer to Lock Pillar Upper Garnish Molding Replacement.
4. Remove the lock pillar lower panel assembly. Refer to Body Lock Pillar Garnish Lower Molding Replacement.
5. Remove the rear seat belt anchor bolts. Refer to Rear Seat Belt Replacement. Release escutcheon, then feed escutcheon and webbing through opening in rear shelf.
6. Lift the front forward edge of the shelf trim upward.
7. Release the 2 rear window shelf trim retaining clips which are accessible from the rear compartment of the vehicle.

1 | Rear Window Shelf Trim Assembly
2 | Rear Window Shelf Trim Clip