For 1990-2009 cars

### Removal Procedure

1. Remove the right instrument panel (I/P) trim panel. Refer to Instrument Panel Trim Panel Replacement - Right Side .
2. Remove the outer air duct screw and duct.

### Installation Procedure

1. Install the outer air duct.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the outer air duct screw.

Tighten
Tighten the air outlet duct screw to 2.5 N·m (22 lb in).

3. Install the I/P trim panel. Refer to Instrument Panel Trim Panel Replacement - Right Side .