For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt tensioner. Refer to Drive Belt Tensioner Replacement.
2. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement.
3. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
4. Remove the windshield washer solvent reservoir. Refer to Windshield Washer Solvent Container Replacement.
5. Install the engine support fixture. Refer to Engine Support Fixture.
6. Remove the engine mount to bracket bolts.
7. Remove the engine mount to side rail nuts.
8. Remove the engine mount from the engine compartment.
9. Remove the engine mount bracket to engine bolts.
10. Remove the engine mount bracket.
11. Remove the engine front cover to water pump bolt.
12. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
13. Remove the engine front cover bolts.
14. Remove the engine front cover.
15. Remove and discard the engine front cover gasket.

### Installation Procedure

1. Install a NEW engine front cover gasket to the dowel pins.
2. Install the engine front cover.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the engine front cover bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

4. Lower the vehicle.
5. Install the engine front cover to water pump bolt.

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

6. Position the engine mount bracket to the engine.
7. Install the engine mount bracket bolts in the following locations.

- | The long bolts in the forward and lower rear holes

- | The short bolt in the upper rear hole

8. Tighten the engine mount bracket bolts in the following sequence.

8.1. | Upper rear

8.2. | Lower rear

8.3. | Forward

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

9. Install the engine mount to the engine compartment.
10. Install the engine mount to side rail nuts.

Tighten
Tighten the nuts to 100 N·m (74 lb ft).

11. Install the engine mount to bracket bolts.
12. Tighten the engine mount to bracket bolts in the following sequence.

12.1. | Middle

12.2. | Rear

12.3. | Front

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

13. Remove the engine support fixture. Refer to Engine Support Fixture.
14. Install the windshield washer solvent reservoir. Refer to Windshield Washer Solvent Container Replacement.
15. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
16. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement.
17. Install the drive belt tensioner. Refer to Drive Belt Tensioner Replacement.