For 1990-2009 cars

### Special Tools

• | EN-38122-A Crankshaft Balancer Holder

• | EN-43653 Flywheel Holding Tool

For equivalent regional tools, refer to Special Tools.

Note: EN-43653 flywheel holding tool may be used instead of EN-38122-A crankshaft balancer holder to prevent crankshaft rotation.

1. Install EN-38122-A holder (1).
2. Remove the balancer retaining bolt and washer. Use EN-38122-A holder and a breaker bar to prevent the crankshaft from rotating when loosening the bolt. Discard the bolt.
3. Remove the crankshaft balancer assembly (1) using a universal removal tool.