For 1990-2009 cars

## Front Brake Hose Replacement Without RPO LNF

Callout | Component Name
--- | ---
Caution: Refer to Bleed Procedure Caution in the Preface section. Caution: Refer to Brake Fluid Irritant Caution in the Preface section. Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

#### Preliminary Procedure

Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .

1 | Brake Pipe Fitting Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Cap or plug the brake pipe fitting to prevent brake fluid loss and contamination.
2. After the installation is complete, bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .

Tighten
19 N·m (14 lb ft)

2 | Brake Hose Bracket Bolt Tighten 25 N·m (35 lb ft)
3 | Brake Hose Tip The brake hose bracket and retaining clip are replaced as an assembly with the brake hose.
4 | Brake Hose Fitting Bolt Tighten 48 N·m (35 lb ft)
5 | Brake Hose Gasket (Qty: 2)

#### Procedure

1. Discard the brake hose gaskets.
2. During assembly, install new brake hose gaskets.

## Front Brake Hose Replacement With RPO LNF

### Removal Procedure

Caution: Refer to Brake Dust Caution in the Preface section.

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Disconnect the front brake pipe fitting (1).

Cap the brake pipe fitting to prevent brake fluid loss and contamination.

4. Remove the front brake hose bracket bolt (1).
5. Remove the brake hose fitting bolt (1).
6. Remove the brake hose fitting gaskets (2) from the brake hose (3).

Discard the brake hose fitting gaskets.

7. Remove the brake hose.

### Installation Procedure

1. Assemble the brake hose fitting bolt (1) with 2 new brake hose fitting gaskets (2) to the brake hose (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the brake hose assembly to the caliper.

Tighten
Tighten the brake hose fitting bolt to 40 N·m (30 lb ft).

3. Install the front brake hose bracket bolt (1).

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

4. Connect the front brake pipe fitting (1).

Tighten
Tighten the fitting to 19 N·m (14 lb ft).

5. Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .
6. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .