For 1990-2009 cars

### Removal Procedure

1. Remove the left headlamp housing bracket. Refer to Headlamp Replacement .
2. Disconnect the horn electrical connector.
3. Remove the horn bracket bolt (1).
4. Remove the horn (2) from the front frame rail.

### Installation Procedure

1. Position the horn (2) into the slot in the front frame rail.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the horn bracket bolt (1).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the horn electrical connector.
4. Install the left headlamp housing bracket. Refer to Headlamp Replacement .