For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Lower the rear axle in order to gain access to the top portion of the rear springs. Refer to Coil Spring Replacement .
3. Remove the upper spring seat/jounce bumper from the spring, while leaving the lower spring seat on the axle.

### Installation Procedure

Important: The rear springs are indexed with the colored tag toward the rear of the vehicle. No up/down or side to side orientation is required.

1. Install the upper spring seat/jounce bumper on the spring.
2. Raise the rear axle in order to seat rear spring. Refer to Coil Spring Replacement .
3. Lower the vehicle.