For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Remove all the air from the hydraulic brake system anytime the hydraulic brake system is opened for repair. The entire bleeding procedure must be followed. Failure to remove all the air in the hydraulic brake system will result in reduced braking performance and possible personal injury.

Warning: Refer to Brake Fluid Irritant Warning in the Preface section.

Caution: Refer to Brake Fluid Effects on Paint and Electrical Components Caution in the Preface section.

1 | Brake Pipe Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip

• | Mark the brake pipes in order to correctly install the pipes to the original positions prior to removal.

• | Cap or plug the brake pipes to prevent fluid loss and contamination.

Tighten
19 N·m (14 lb ft)

2 | Brake Pipe Nut (Qty: 4) Tip

• | Mark the brake pipes in order to correctly install the pipes to the original positions prior to removal.

• | Cap or plug the brake pipes to prevent fluid loss and contamination.

• | Bleed the brake system anytime the system is opened for repairs. Refer to Hydraulic Brake System Bleeding.

Tighten
19 N·m (14 lb ft)

3 | Valve Bracket Assembly Bolt Tip Loosen bolt but do not remove. Tighten 25 N·m (18 lb ft)
4 | Valve Bracket Assembly Bolt Tighten 25 N·m (18 lb ft)
5 | Proportioning Valve Tip Slide the bracket assembly upward in order to remove from frame rail.