For 1990-2009 cars

### EBCM Replacement

If the electronic brake control module (EBCM) is replaced, the following procedures must be performed:

EBCM Reprogramming--Refer to Service Programming System (SPS).

### EBCM Reprogramming

If the EBCM needs to be reprogrammed, refer to Service Programming System (SPS).

### Setup for Component Replacement

The replacement of some components will require a setup procedure for complete repair.

• | Brake Pressure Modulator Valve Replacement

• | Electronic Brake Control Module (EBCM) programming or replacement

• | Steering angle sensor replacement

• | Steering column replacement

• | Steering column replacement

• | Steering gear replacement

• | Yaw rate and Lateral accelerometer sensor

1. Center the steering wheel with the wheels facing forward.
2. With a scan tool, perform the special functions steering position sensor calibration and follow the on screen instructions.