For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the turn signal switch bracket. Refer to Turn Signal Switch Bracket Replacement.

1 | Ignition Lock Cylinder Case Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Use a hammer and chisel to bite into the shear bolt at a position offset from center and tap the chisel to rotate the bolt in order to remove it.
2. Torque the new ignition lock cylinder case bolt until the head shears off.

2 | Ignition Lock Cylinder Case

#### Procedure

1. Disconnect any electrical connectors as needed.
2. The ignition lock cylinder must be in the RUN position to remove the ignition lock cylinder case.
3. If the ignition lock cylinder is stuck in the OFF position with the lock bolt engaged then proceed to cut off the lock cylinder housing collar at the points shown in the graphic.
4. Transfer any parts as needed.