For 1990-2009 cars

#### Special Tools

• | 83 90 114 Sleeve

• | 83 90 312 Drift, Bearing Race Input Shaft

• | 87 91 311 Sleeve, Bearing Driver Shaft

• | 87 92 210 Support, Differential Bearing

• | 87 92 236 Support

• | J 44809 Output Shaft Seal Installer

1. Press in the new differential bearing race using the J 44809 . Use the 87 92 236 as a base for the pressing operation.
2. Install the new axle using the J 44809 .
3. Press in the new input shaft bearing race using the 83 90 312 (1). Use the 83 90 114 (2) and the 87 91 311 (3) as a base for the pressing operation.