For 1990-2009 cars

## Seat Belt Retractor Pretensioner Replacement - Front Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

Disable the SIR in Zones 2 or 6. Refer to SIR Disabling and Enabling .

1 | Seat Belt Anchor Bolt Notice: Refer to Fastener Notice in the Preface section. Tip Move the seat to the full forward position to gain access to the bolt. Tighten
45 N·m (33 lb ft)

2 | Seat Belt Adjuster Cover
3 | Seat Belt Adjuster Bolt Tighten 45 N·m (33 lb ft)
4 | Seat Belt Retractor Bolt Tip Remove the center pillar lower trim panel to gain access to the bolt. Refer to Center Pillar Lower Garnish Molding Replacement . Tighten 45 N·m (33 lb ft)
5 | Front Seat Belt Retractor Assembly Tip Disconnect the belt tension sensor electrical connector.