For 1990-2009 cars

### Removal Procedure

1. Remove the turbocharger. Refer to Turbocharger Replacement .
2. Remove the oil return pipe (1).
3. Remove the oil return pipe o-ring (2) and gasket (3).

### Installation Procedure

1. Lubricate and install a NEW turbocharger oil return pipe gasket (3) and o-ring (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the turbocharger oil return pipe (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the turbocharger. Refer to Turbocharger Replacement .