For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Side Door Upper Hinge Assembly Replacement

1 | Front Side Door Hinge Upper Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip: Replace only one hinge at a time. Tighten
35 N·m (26 lb ft)

2 | Front Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Front Side Door Upper Hinge Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

#### Procedure

Check the door for proper alignment, adjust as necessary.

#### Front Side Door Lower Hinge Assembly Replacement

4 | Front Side Door Hinge Lower Bolt (Qty: 2) Tip: Replace only one hinge at a time. Tighten 35 N·m (26 lb ft)
5 | Front Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
6 | Front Side Door Lower Hinge Assembly Notice: Striker alignment is a crucial part of door latch operation. Do not use the door striker to adjust the door to the vehicle. Failure to properly adjust the striker can result in damage to the door latch and the striker.

#### Procedure

Check the door for proper alignment, adjust as necessary.