For 1990-2009 cars

#### Tools Required

J 38122-A Harmonic Balancer Holder

### Removal Procedure

1. Remove the engine drive belt. Refer to Drive Belt Replacement .
2. Use J 38122-A to prevent the crankshaft from rotating while loosening the crankshaft balancer bolt.
3. Remove the crankshaft balancer bolt. Discard the bolt.
4. Remove the crankshaft balancer.

### Installation Procedure

1. Install the crankshaft balancer.
2. Install a NEW crankshaft balancer bolt.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Use J 38122-A to prevent the crankshaft from rotating while tightening the crankshaft balancer bolt.

Tighten
Tighten the bolt to 100 N·m (74 lb ft) plus 75 degrees.

4. Install the engine drive belt. Refer to Drive Belt Replacement .